{ "" "" "" "Vip.Mixer: The MixerII register map changed in ACDS v16.0. Please refer to the VIP User Guide for details." {  } {  } 0 12251 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Vip.Reset_Source.reset_sys: Associated reset sinks not declared" {  } {  } 0 12251 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Vip.Reset_Source.reset_warm: Associated reset sinks not declared" {  } {  } 0 12251 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Vip.Reset_Source.reset_cold: Associated reset sinks not declared" {  } {  } 0 12251 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Vip.Video_Output.control: Interrupt sender control.av_mm_control_interrupt is not connected to an interrupt receiver" {  } {  } 0 12251 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Vip.Video_Output: Interrupt sender Video_Output.status_update_irq is not connected to an interrupt receiver" {  } {  } 0 12251 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Vip.: You have exported the interface HPS.f2h_sdram1_data but not its associated reset interface.  Export the driver(s) of HPS.h2f_reset" {  } {  } 0 12251 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Vip.: You have exported the interface HPS.f2h_sdram2_data but not its associated reset interface.  Export the driver(s) of HPS.h2f_reset" {  } {  } 0 12251 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Variable or input pin \"data_b\" is defined but never used." {  } {  } 0 287013 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Variable or input pin \"data_a\" is defined but never used." {  } {  } 0 287013 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Port \"extclk\" on the entity instantiation of \"cyclonev_pll\" is connected to a signal of width 1. The formal width of the signal in the module is 2.  The extra bits will be left dangling without any fan-out logic." {  } {  } 0 12030 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Port \"trs\" on the entity instantiation of \"statemachine\" is connected to a signal of width 2. The formal width of the signal in the module is 1.  The extra bits will be ignored." {  } {  } 0 12020 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Port \"reset_value\" on the entity instantiation of \"h_counter\" is connected to a signal of width 32. The formal width of the signal in the module is 16.  The extra bits will be ignored." {  } {  } 0 12020 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Overwriting existing clock: vip\|hps\|fpga_interfaces\|clocks_resets\|h2f_user0_clk" {  } {  } 0 332043 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "LOCKED port on the PLL is not properly connected on instance \"emu:emu\|pll:pll\|pll_0002:pll_inst\|altera_pll:altera_pll_i\|general\[0\].gpll\". The LOCKED port on the PLL should be connected when the FBOUTCLK port is connected. Although it is unnecessary to connect the LOCKED signal, any logic driven off of an output clock of the PLL will not know when the PLL is locked and ready." {  } {  } 0 21300 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "Vip.vip: Module dependency loop involving: \"HPS\"" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "alt_vip_common_frame_counter.v" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "alt_vip_cvo_mode_banks.sv" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "altera_pll.v" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "altera_cyclonev_pll.v" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "altera_pll_reconfig_core.v" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "genlock_enable_sync" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "u_calculate_mode" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "mode_banks" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "RST port on the PLL is not properly connected" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "alt_vip_cvo_core.sdc" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "alt_vip_packet_transfer.sdc" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "alt_vip_common_dc_mixed_widths_fifo.sdc" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
{ "" "" "" "vip_HPS_fpga_interfaces.sdc" {  } {  } 0 9999 "" 0 0 "Design Software" 0 -1 0 ""}
