## RGB2SVIDEO

This device converts RGB + Sync analog signal to S-Video (and also Composite).
Both PAL and NTSC supported (you should choose one at build).

PCB size: 37.2x16.4mm

[![photo](out/pcb3d-top.rev.A2.webp)](out/pcb3d-top.rev.A2.webp?raw=true)
[![photo](out/pcb3d-bottom.rev.A2.webp)](out/pcb3d-bottom.rev.A2.webp?raw=true) 
